{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":25,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["Groundwater physico-chemical analyses"]
["Sample_id","Treatment Plant","Sampling Point Abbreviation","Alcalinity (mg/L)","Colour (CU)","Conductivity at 20°C (µS/cm)","[H+] (pH)","Total hardness (°F)","Index of aggressivity","Dry residue at 180°C (mg/L)","Temperature (°C)","Turbidity (NTU)","Ammonia (µg/L)","Chlorites (µg/L)","Chlorides (mg/L)","Fluoride (mg/L)","Phosphate (mg/L)","Nitrate (mg/L)","Nitrite (µg/L)","Sulphate (mg/L)","Calcium (mg/L)","Iron (µg/L)","Magnesium (mg/L)","Volatile Organic Compounds (VOC) (µg/L)","Polycyclic Aromatic Hydrocarbons (PAH) (ng/L)"]
["3A","Site 1","Aquifer",200.0,0.0,716.0,7.36,30.0,12.14,465.40000000000003,14.6,"<0.010","<0,10","<0.02",30.0189,"<0,5","<0,20",40.727,"<0.20",57.3311,97.0,"<5",22.0,27.0,"<2.00"]
["4A","Site 1","Aquifer",180.94,"<0.01",689.119,7.64,32.31,12.4,447.927,14.3,"<0.010","<0.10","<0.02",27.91,"<0.50","<0.20",37.56,"<0.20",52.6,101.0,6.0,22.1,27.0,"<2.00"]
["5A","Site 1","Aquifer",174.28,"<0.01",720.201,7.69,28.69,12.34,468.131,13.8,"<0.010","<0.10","<0.02",29.33,"<0.50","<0.20",38.61,"<0.20",54.5,98.27,11.0,21.6,25.0,"<2.00"]
["6A","Site 1","Aquifer",224.94,"<0.01",717.68,8.04,33.0,12.26,466.492,15.1,"<0.010","<0.10","<0.02",27.88,"<0.50","<0.20",35.82,"<0.20",52.0,97.73,5.0,19.5,31.0,"<2.00"]
["7A","Site 1","Aquifer",210.58,"<0.01",728.947,7.62,29.21,12.41,473.816,15.2,"<0.010","<0.10","<0.02",29.38,"<0.50","<0.20",38.08,"<0.20",54.0,120.1,"<5",19.9,27.0,"<2.00"]
["8A","Site 1","Aquifer",207.57,"<0.01",702.467,7.55,28.99,12.33,456.604,15.5,"<0.010","<0.10","<0.02",27.81,"<0.50","<0.20",38.0,"<0.20",53.2,87.6,"<5",22.9,26.0,"<2.00"]
["9A","Site 1","Aquifer",207.34,"<0.01",711.002,7.64,26.15,12.37,462.151,17.1,"<0.010","<0.10","<0.02",27.39,"<0.50","<0.20",37.28,"<0.20",52.0,87.46,"<5",22.0,17.0,"<2.00"]
["10A","Site 1","Aquifer",193.95,"<0.01",732.79,7.62,28.34,12.36,476.314,17.0,"<0.010","<0.10","<0.02",29.83,"<0.50","<0.20",37.91,"<0.20",55.5,91.7,"<5",17.8,24.0,"<2.00"]
["11A","Site 1","Aquifer","NA","<0.01","NA",7.7,"NA",12.35,476.314,15.5,"<0.010","<0.10","<0.02",28.01,"<0.50","<0.20",37.91,"<0.20","NA","NA","NA","NA","NA","NA"]
["12A","Site 1","Aquifer",206.69,"<0.01",735.464,7.77,27.32,12.53,478.052,15.1,"<0.010","<0.10","<0.02",28.01,"<0.50","<0.20",39.6,"<0.20",53.3,85.25,"<5",19.8,28.0,3.04]
["13A","Site 1","Aquifer",212.17,"<0.01",730.142,7.81,26.91,12.57,474.592,15.2,"<0.010","<0.10","<0.02",28.49,"<0.50","<0.20",37.56,"<0.20",54.2,92.49,7.0,21.8,23.0,"<2.00"]
["14A","Site 1","Aquifer",205.37,"<0.01",715.958,7.74,26.55,12.47,465.373,15.5,"<0.010","<0.10","<0.02",27.9,"<0.50","<0.20",38.41,"<0.20",51.5,85.55,"<5",20.9,17.0,"<2.00"]
["1A_cr","Site 2","Aquifer",203.81,"<0.01",727.981,7.77,27.41,12.51,473.188,15.1,"<0.010","<0.10","<0.02",30.52,"<0.50","<0.20",43.04,"<0.20",51.0,93.55,17.0,20.0,11.0,"<2.00"]
["2A_cr","Site 2","Aquifer",207.82,"<0.01",729.129,7.64,27.75,12.4,473.934,15.2,"<0.010","<0.10","<0.02",30.33,"<0.50","<0.20",41.85,"<0.20",50.3,96.07,10.0,20.0,14.0,"<2.00"]