{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":18,"n_cols":2,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
["Marker","Freq."]
["POLE4",0.677068723702665]
["ICB resistance signature 1",0.64726507713885]
["TIDE",0.607293127629734]
["POLE",0.593267882187938]
["AXL pathway",0.562061711079944]
["ICB resistance signature 2",0.524894810659187]
["POLE2",0.454417952314165]
["IPS",0.409887798036466]
["ICB resistance signature 3",0.384291725105189]
["CD274",0.35273492286115]
["mut. load",0.334852734922861]
["AXL",0.322230014025245]
["POLE3",0.271037868162693]
["PDCD1LG2",0.260168302945302]
["IFN-y (reduced set)",0.253506311360449]
["IFN-y (expanded set)",0.246493688639551]
["CTLA4",0.237026647966339]