{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["工作表1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"工作表1","index":0,"n_rows":8,"n_cols":4,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["Table S2. Separation gradient of high pH reversed phase chromatography. "]
[]
["Time (min)","A (98% H2O, pH 10)","B (98% ACN, pH 10) ","Speed（μL/min）"]
[0,1,0,700]
[3,1,0,700]
[5,0.95,0.05,700]
[45,0.65,0.35,700]
[53,0.1,0.9,700]