{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":25,"rows_kept":16,"cut":false,"hidden":false,"merged":[]}
["Post-chlorination water physico-chemical analyses"]
["Sample_ID","Treatment Plant","Sampling Site","Alcalinity (mg/L)","Cl2 (mg/L)","Colour (CU)","Conductivity at 20°C (µS/cm)","[H+] (pH)","Total hardness (°F)","Index of aggressivity","Dry residue at 180°C (mg/L)","Temperature (°C)","Turbidity (NTU)","Ammonia (µg/L)","Chlorites (µg/L)","Chlorides (mg/L)","Fluoride (mg/L)","Phosphate (mg/L)","Nitrate (mg/L)","Nitrite (µg/L)","Sulphate (mg/L)","Calcium (mg/L)","Iron (µg/L)","Magnesium (mg/L)","Volatile Organic Compounds (VOC) (µg/L)"]
["3C","Site 1","Chlor",203.0,0.02,0.19,704.0,7.45,28.0,12.38,457.6,12.9,0.06,"<0.10","<200",29.25,"<0.5","<0.20",39.77,"<0.10",56.38,102.0,5.0,21.0,"NA"]
["4C","Site 1","Chlor",171.56,0.03,"<0.01",617309.0,7.65,30.01,12.36,401.251,12.9,"<0.010","<0.10","<0.02",28.37,"<0.50",1.14,38.65,"<0.20",53.5,97.08,20.0,23.9,8.0]
["5C","Site 1","Chlor",172.05,0.01,"<0.01",703086.0,7.6,28.57,12.25,457.006,14.5,"<0.010","<0.10","<0.02",28.82,"<0.50","<0.20",37.02,"<0.20",53.4,99.39,"<5",20.9,10.0]
["6C","Site 1","Chlor",221.74,0.01,"<0.01",702726.0,7.81,"NA","NA",456.772,14.7,"<0.010","<0.10",0.2,28.21,"<0.50",11596.0,37.29,"<0.20",53.0,112.2,"<5",21.1,11.0]
["7C","Site 1","Chlor",209.66,0.02,"<0.01",724798.0,7.63,29.15,12.42,471.119,15.6,"<0.010","<0.10","<0.02",27.87,"<0.50",0.82,38.5,"<0.20",52.6,106.9,6.0,21.6,11.0]
["8C","Site 1","Chlor",207.59,0.02,"<0.01",680313.0,7.66,"<0.01","<1.00",442.203,16.0,"<0.010","<0.10","<0.02",28.58,"<0.50","<0.20",37.78,"<0.20",53.3,89.31,"<5",20.9,11.0]
["9C","Site 1","Chlor",207.52,0.04,"<0.01",700165.0,7.53,29.48,12.32,455.107,16.3,"<0.010","<0.10","<0.02",28.9,"<0.50","<0.20",37.81,"<0.20",53.1,94.79,"<5",21.2,11.0]
["10C","Site 1","Chlor",191.08,0.01,"<0.01",697342.0,7.52,31.87,12.31,453.272,17.7,"<0.010","<0.10","<0.02",28.6,"<0.50","<0.20",38.77,"<0.20",53.6,98.31,"<5",20.1,11.0]
["11C","Site 1","Chlor",210.94,0.0,"<0.01",725479.0,7.38,33.09,12.23,471.561,18.8,"<0.010","<0.10","<0.02",30.26,"<0.50","<0.20",42.57,"<0.20",55.4,167.0,42.0,21.8,7.0]
["12C","Site 1","Chlor",210.21,0.09,"<0.01",715535.0,7.61,28.02,12.38,465.098,16.3,"<0.010","<0.10","<0.02",28.92,"<0.50","<0.20",39.04,"<0.20",54.1,88.45,"<5",21.7,14.0]
["13C","Site 1","Chlor",201.82,0.1,"<0.01",703133.0,7.71,30.11,12.5,457.036,15.8,"<0.010","<0.10","<0.02",27.95,"<0.50","<0.20",37.8,"<0.20",51.5,88.24,9.0,21.3,11.0]
["14C","Site 1","Chlor",204.95,0.24,"<0.01",704303.0,7.66,32.21,12.48,457.797,14.9,"<0.010","<0.10","<0.02",28.84,"<0.50","<0.20",39.77,"<0.20",53.0,92.71,7.0,19.9,2.0]
["1C_cr","Site 2","Chlor",202.33,0.1,"<0.01",716098.0,7.59,31.36,12.39,465.464,15.5,"<0.010","<0.10","<0.02",29.84,"<0.50","<0.20",42.32,"<0.20",50.5,96.05,"<5",20.8,9.0]
["2C_cr","Site 2","Chlor",199.06,0.03,"<0.01",698868.0,7.57,32.35,12.38,454.264,14.9,"<0.010","<0.10","<0.02",29.55,"<0.50","<0.20",41.29,"<0.20",49.6,97.53,"NA",19.2,7.0]